{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"電流",{"$f":"IF(AND(ISNUMBER(D5),ISNUMBER(D7)),REPT(\" \",10)&ROUND(D5/D7,2),\"\")","v":""},10,"A"]
[]
[null,"電力",{"$f":"IF(AND(ISNUMBER(D3),ISNUMBER(D7)),REPT(\" \",10)&ROUND(D3*D7,2),\"\")","v":""},200,"W"]
[]
[null,"電圧",{"$f":"IF(AND(ISNUMBER(D3),ISNUMBER(D5)),REPT(\" \",10)&ROUND(D5/D3,2),\"\")","v":"          20"},null,"V"]

{"sheet":"Sheet2","index":1,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"電流",10,"A"]
[]
[null,"電力",200,"W"]
[]
[null,"電圧",20,"V"]